**Soffit element Duo LE**

Soffit element for fitting in the window soffit.

Is required as compulsory accessory when installing in the window soffit.

Technical data

|  |  |
| --- | --- |
| Article: | Duo LE |
| Air flow volume: | 60 m³/h |
| Material: | Aluminium |
| Colour: | Aluminium, not painted |
| Weight: | 2,16 kg |
| Weight including packaging: | 2,79 kg |
| Width: | 920 mm |
| Height: | 410 mm |
| Depth: | 64 mm |
| Width with packaging: | 1.020 mm |
| Height with packaging: | 460 mm |
| Depth with packaging: | 110 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799930877 |
| Article number: | 0093.0087 |

Manufacturer: MAICO

Duo LE Soffit element