**Circuit board PL ER 100 VZ 15**

Circuit board as spare part for ER 100 VZ 15 fan insert.

For model with time delay switch 15 min. overrun time.

Technical data

|  |  |
| --- | --- |
| Article: | PL ER 100 VZ 15 |
| Weight: | 0,03 kg |
| Weight including packaging: | 0,11 kg |
| Width: | 65 mm |
| Height: | 25 mm |
| Depth: | 115 mm |
| Width with packaging: | 150 mm |
| Height with packaging: | 45 mm |
| Depth with packaging: | 210 mm |
| Range: | B |
| GTIN (EAN): | 4012799100416 |
| Article number: | E101.1025.9001 |

Manufacturer: MAICO

PL ER 100 VZ 15 Circuit board