**Air filter, replacement ZF 60/100**

ZF 60/100: Replacement air filter for ER... and ER-AP/ER-APB... fan inserts and Centro... exhaust air elements.

Technical data

|  |  |
| --- | --- |
| Article: | ZF 60/100 |
| Installation position: | vertical / horizontal |
| Weight: | 0,002 kg |
| Weight including packaging: | 0,022 kg |
| Filter class: | G2 |
| Width: | 135 mm |
| Height: | 135 mm |
| Depth: | 8 mm |
| Width with packaging: | 280 mm |
| Height with packaging: | 200 mm |
| Depth with packaging: | 20 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 5 pieces |
| Range: | B |
| GTIN (EAN): | 4012799936800 |
| Article number: | 0093.0680 |

Manufacturer: MAICO

ZF 60/100 Air filter, replacement