**Roof socket for flat roofs, tiltable SOK 25**

Flat roof socket for assembly of roof fans.

With tilting device to move the fan out of the way when working on the ventilation duct.

With sound and heat insulation made of abrasion-resistant and non-flammable mineral fibre plates.

Recommended accessories: SZ intermediate sockets.

Technical data

|  |  |
| --- | --- |
| Article: | SOK 25 |
| Housing material: | Sheet steel, galvanised |
| Weight: | 14,56 kg |
| Weight including packaging: | 14,6 kg |
| Swivellable: | ✔ |
| Suitable for nominal size: | 250 mm |
| Width: | 845 mm |
| Height: | 290 mm |
| Depth: | 845 mm |
| Width with packaging: | 845 mm |
| Height with packaging: | 290 mm |
| Depth with packaging: | 845 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799939924 |
| Article number: | 0093.0992 |

Manufacturer: MAICO

SOK 25 Roof socket for flat roofs, tiltable