**Aeronom room air system FKV 125**

Flat channel system for domestic ventilation.

Channel dimension: 150 mm x 80 mm.

Quick and easy installation.

Technical data

|  |  |
| --- | --- |
| Article: | FKV 125 |
| Type of installation: | Recessed-mounted |
| Material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,09 |
| Weight including packaging: | 0,1 kg |
| Channel dimension: | 150 mm x 80 mm |
| Hydraulic diameter: | 72 mm |
| Width with packaging: | 155 mm |
| Height with packaging: | 10 mm |
| Depth with packaging: | 85 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799780151 |
| Article number: | 0078.0015 |

Manufacturer: MAICO

FKV 125 Aeronom room air system