**Counter flange GFI 63**

Counter flange for connection between the fan and the duct.

Bore holes according to the ISO 6580 standard.

Technical data

|  |  |
| --- | --- |
| Article: | GFI 63 |
| Material: | Sheet steel |
| Colour: | grey |
| Weight: | 2,7 kg |
| Weight including packaging: | 2,7 kg |
| Suitable for nominal size: | 630 mm |
| Width: | 720 mm |
| Height: | 720 mm |
| Depth: | 5 mm |
| Width with packaging: | 720 mm |
| Height with packaging: | 720 mm |
| Depth with packaging: | 5 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799732594 |
| Article number: | 0073.0259 |

Manufacturer: MAICO

GFI 63 Counter flange